1. It is OK to mix radial and bias ply tires on a truck providing the part of a dual wheel assembly.

  True  False

|  |
| --- |
| 1. What steps should you take when inflating a tube tire?
 |
|  |  |
|  |  |
|  |  |
|  |  |

|  |
| --- |
| 1. Name an item of mandatory Personal Protective Equipment (PPE) that is always required when working on tire servicing.
 |
|  |  |
|  |  |

|  |
| --- |
| 1. Name three faults you would look for when inspecting wheel parts.
 |
| i. |  |
| ii. |  |
| iii. |  |

5. The wheel nuts on a newly inflated wheel should be checked and re-torqued after 80 to 160 kms.

  True  False

1. It is OK to mix radial and bias ply tires on a truck providing the part of a dual wheel assembly.

False

1. What steps should you take when inflating a tube tire?

If a tube is used the tire must be inflated to full pressure, deflated and re-inflated to ensure no localized stresses on the tube.

1. Name an item of mandatory Personal Protective Equipment (PPE) that is always required when working on tire servicing.

Safety Footwear

1. Name three faults you would look for when inspecting wheel parts.

Any two of:

* Sprung side/lock rings
* Cracked rings/rims
* Bent flanges
* Tool marks
* Loss of contour
* Metal thickness of the mating surfaces
1. The wheel nuts on a newly inflated wheel should be checked and re-torqued after 80 to 160 kms.

 True